Device: Patchpanel B-Br-Keller/SM/M-Br

Role: Patchpanel Glas Singlemode

Site: Block B

Networking

Front Port	Description	Patched to	Rear Port
duplex-port-1	Patchpanel B-Br-Keller ↔ A-Br-Keller / duplex-port-1	Rear / 1
duplex-port-2	b-switch-10 / 51	Rear / 2
duplex-port-3	fahrradwerkstatt-switch-1 / 9	Rear / 3
duplex-port-4	Rear / 4
duplex-port-5	Rear / 5
duplex-port-6	Rear / 6
duplex-port-7	Rear / 7
duplex-port-8	Rear / 8
duplex-port-9	Rear / 9
duplex-port-10	Rear / 10
duplex-port-11	Rear / 11
duplex-port-12	Rear / 12
Rear Port	Description	Patched to
Rear	Patchpanel M-Br/SM/B-Br / Rear